CHECK LIST BEFORE LEAVING THE BOAT
· Check shackles have been moused with cable ties (if on mooring).
· Shut down engines.
· Raise engines.
· Check fuel in tanks – is there enough for next time?
· Close breather vents in tanks.
· Turn off and remove engine circuit breaker keys and put them in top pocket of tool box.
· Switch off all instruments on panel.
· Turn off house battery circuit breaker key (leave key hanging on cord).
· Replace rubber Raymarine cover on plotter.
· Close side window (if open).
· Remove ignition keys.
· Check all flags have been lowered and stowed.
· Return life ring to cabin.
· Return yellow buoy (from main mooring rope) to cabin.
· Lock cabin and toilet doors.
· Wash down decks and return brush and bucket to fish locker.
· Lock fish locker.
· Ensure gunwhale door is securely closed.
Please report any faults/issues to Colin Smith - 07742 783085 


